**The update firmware instructions for MPS-850**

MPS-850 module can use USB flash drive to update the firmware. The USB flash drive should be formatted as "FAT32" before update.

The update firmware should be named "SOUNDS.DAT".


The firmware should be located the "UPDATE" folder of the USB flash drive.

Operation:

1. Both press the [KIT] and [SONG] buttons and then turn on the module. If the module doesn't find USB flash drive, the LCD will display "NO FILE" as below.



1. Insert the USB flash drive in the side panel of the module, the module will enter the update menu.



1. Then press the [ENTER] button to start the update. The LED under the [RECORD] and [START/STOP] buttons will begin to flash, indicate the update is going. At this time, please don't turn off the module or pull out the USB flash drive.

After finish, the module will enter the update menu again, waiting for next update.

1. When you finish update, press the [POWER] button to turn off the module, remove the USB drive, and then restart the module.

1. We suggest to restore the factory settings after updating the software (all of user data will be lost)
2. You can restore the factory set by following steps:  
   a) Press the [<] and [>] buttons simultaneously.  
   b) Press [POWER] button.

c) Until the LCD displays “Factory Resetting…”. Complete reset operation, the module will return to the KIT MENU.